; Copyright (c) 2012 Microsoft
;
; Module Name: EisMultiplexerWinDriver.inf
; Description: Installation inf for EisMultiplexer device.
;
; THIS CODE AND INFORMATION IS PROVIDED "AS IS" WITHOUT WARRANTY OF ANY
; KIND, EITHER EXPRESSED OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE
; IMPLIED WARRANTIES OF MERCHANTABILITY AND/OR FITNESS FOR A PARTICULAR
; PURPOSE.

[Strings]
DeviceName = "EisMultiplexer"
VendorName = "RHD"
SourceName = "EisMultiplexer Install Disk"
DeviceID   = "VID_FE17&PID_07DC"
DeviceGUID = "{FE5A454B-A699-7694-FF47-75CA5F56013E}"

[Version]
Signature   = "$Windows NT$"
Class       = "Universal Serial Bus devices"
ClassGuid   = {88BAE032-5A81-49F0-BC3D-A4FF138216D6}
Provider    = "Microsoft"
CatalogFile = EisMultiplexerWinDriver.cat
DriverVer   = 04/09/2017, 6.1.7600.16385
DriverPackageDisplayName = "EisMultiplexer"

[ClassInstall32]
Addreg = WUsb_Class_AddReg

[WUsb_Class_AddReg]
HKR,,,0,"Universal Serial Bus devices"
HKR,,Icon,,-20

; ============== Device section =================
[Manufacturer]
%VendorName% = WUsb_DeviceGroup,NTX86,NTAMD64

[WUsb_DeviceGroup.NTX86]
%DeviceName% = WUsb_Device, USB\%DeviceID%

[WUsb_DeviceGroup.NTAMD64]
%DeviceName% = WUsb_Device, USB\%DeviceID%

[WUsb_Device.NT.HW]
AddReg=WUsb_Device_AddReg

[WUsb_Device.NTAMD64.HW]
AddReg=WUsb_Device_AddReg

[WUsb_Device_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,%DeviceGUID%

; ======= Power policy settings (default) ========

; Indicates whether the device is capable of being powered down when idle 
; (Selective Suspend). 
HKR,,DeviceIdleEnabled,0x00010001,1

; Sets the default value of the AUTO_SUSPEND power policy setting. This 
; registry key is used to enable or disable selective suspend when a 
; handle is not open to the device. 
HKR,,DefaultIdleState,0x00010001,0

; Sets the default state of the SUSPEND_DELAY power policy setting. The 
; value indicates the amount of time in milliseconds to wait before 
; determining that a device is idle. 
HKR,,DefaultIdleTimeout,0x00010001,5000

; When set to a nonzero value, it suspends the device even if it does not 
; support RemoteWake. 
HKR,,DeviceIdleIgnoreWakeEnable,0x00010001,0

; Indicates whether a check box should be enabled in the device Properties 
; page that allows a user to override the idle defaults. 
HKR,,UserSetDeviceIdleEnabled,0x00010001,0

; Indicates whether the device should be allowed to wake the system from a
; low power state. 
HKR,,SystemWakeEnabled,0x00010001,0

; ========== Driver/Service setup ==============
[WUsb_Device.NT.Services]
Include    = winusb.inf
AddService = WinUSB,0x00000002,WUsb_AddService

[WUsb_Device.NTAMD64.Services]
Include    = winusb.inf
AddService = WinUSB,0x00000002,WUsb_AddService

[WUsb_AddService]
DisplayName   = "WinUSB - Kernel Driver 04/09/2017 6.1.7600.16385"
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\WinUSB.sys

; =========== Sources/Destinations ==============
[SourceDisksNames]
1 = %SourceName%

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1,x86
WdfCoInstaller01009.dll = 1,x86
libusbK_x86.dll = 1,x86

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 1,amd64
WdfCoInstaller01009.dll = 1,amd64
libusbK.dll     = 1,amd64
libusbK_x86.dll = 1,x86

[DestinationDirs]
CoInstallers_CopyFiles = 11
libusb_files_dll       = 10,system32
libusb_files_dll_wow64 = 10,syswow64
libusb_files_dll_x86   = 10,system32

[libusb_files_dll]
libusbK.dll

[libusb_files_dll_x86]
libusbK.dll, libusbK_x86.dll

[libusb_files_dll_wow64]
libusbK.dll, libusbK_x86.dll

[WUsb_Device.NT]
Include = winusb.inf
Needs   = WINUSB.NT
CopyFiles = libusb_files_dll_x86

[WUsb_Device.NTAMD64]
Include = winusb.inf
Needs   = WINUSB.NT
CopyFiles = libusb_files_dll, libusb_files_dll_wow64

; ========= WDF/CoInstaller section =============
[WUsb_Device.NT.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[WUsb_Device.NTAMD64.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[WUsb_Device.NT.Wdf]
KmdfService = WINUSB, WUsb_wdfsect

[WUsb_Device.NTAMD64.Wdf]
KmdfService = WINUSB, WUsb_wdfsect

[WUsb_wdfsect]
KmdfLibraryVersion = 1.9
